
NTT02 – 24 Hour General Purpose Timeswitch

Product Image & Line Diagram

Technical Data

|  |  |
| --- | --- |
| **General** |  |
| Operating Voltage | 230V AC |
| Frequency | 50Hz |
| Installation Type | Surface or recessed |
| Min Depth of Wall Box | 32mm, Single gang back box or pattress |
| Contact Type | Normally open |
| Class Protection | Class 2 |
| Program | 24 Hour daily program (96 segments, 48 ON, 48 OFF) |
| Number of Channels | 1 |
| Switch Rating | 16A Resistive, 8A Inductive. 1 HP. 750W Incandescent/ |
| Halogen/Fluorescent, 100W CFL lighting. 100W LED Lighting. |
| LED Indicators | Power |
| Advance Function | Permanent ON/OFF or timed only |
| Operating Temperature | 0°C to 40°C |
| Accessories (Included) | Instructions, Fittings |
| Accessories (Optional) | None |
| Dimensions | Height 92mm, Width 92mm, Depth 60mm |
| Construction | Casing: Polycarbonate |
| Weight | 157g |
| EAN | 5012483012307 |
| Designed In Accordance To | BS EN 60730-2-7  Includes updates and amendments. |
| Guarantee Period | 3 Years |