
NTT04 – 24 Hour/7 Day General Purpose Timeswitch

Product Image & Line Diagram

Technical Data

|  |  |
| --- | --- |
| **General** |  |
| Operating Voltage | 230V AC |
| Frequency | 50Hz |
| Installation Type | Surface or recessed |
| Min Depth of Wall Box | 32mm, Single gang back box or pattress |
| Contact Type | Normally open |
| Class Protection | Class 2 |
| Program | 7 Day weekly program (4 ON/OFF per day, 28 ON/OFF per week) |
| Number of Channels | 1 |
| Power Reserve | Yes, 720 Hours (Non-replaceable rechargeable battery) |
| Switch Rating | 16A Resistive, 4A Inductive. 1 HP. 2400W Incandescent/ |
| Halogen. 750W Fluorescent, 100W LED/CFL lighting. |
| LED Indicators | Power, Output |
| Boost Function | Yes, 1 Hour or 2 Hour |
| Advance Function | Yes, Permanent or until next programmed operation |
| Operating Temperature | 0°C to 40°C |
| Accessories (Included) | Instructions, Fittings |
| Accessories (Optional) | None |
| Dimensions | Height 92mm, Width 92mm, Depth 59mm |
| Construction | Casing: Polycarbonate |
| Weight | 168g |
| EAN | 5012483012321 |
| Designed In Accordance To | BS EN 60730-2-7  Includes updates and amendments. |
| Guarantee Period | 3 Years |