
TS900N – 24 Hour Immersion Heater Time Controller

Product Image & Line Diagram



Technical Data

|  |  |
| --- | --- |
| **General** |  |
| Operating Voltage | 230v AC |
| Frequency | 50Hz |
| Installation Type | Surface |
| Switch Rating | 13A Resistive (3kw) 400W filament, 60W fluorescent/CFL lighting. 80W LED Lighting. |
| Operating Temperature | 0°C to +40°C |
| Dimensions | Height 121.5mm, Width 74mm, Depth 41.6mm |
| Weight | 151g Unpacked |
| EAN | 5012483013380 |
| Designed In Accordance To | BS 1363, BS EN 60730-2-7  Includes updates and amendments. |
| Guarantee Period | 3 Years |
|  |  |
| **Functions** | . |
| Timer Mode | 24 Hour |
| Programs | 24 on/off times per day, minimum on/off time between setting 30minutes |
| Manual Override | Self-cancelling to the next program change |
|  |  |
| **Construction** |  |
| Casing | Polycarbonate |